HOW TO RESET EPSON WASTE INKPAD COUNTER:

1.	Open AdjProgcracked.exe.

2.	Click “Select”.

3.	Select Model Name: Your printer model

4.	Select Port: USB___ (Your printer model)

5.	Click OK.

6.	Click Particular adjustment mode.

7.	Select Waste ink pad counter. Click OK.

8.	Click Check. It should show 100% or more.

9.	Click the check box beside Main paid counter. 
 
10.	Click Initialization. Done. Reboot printer. 

Then check main pad counter again. Should be zero now. Thanks!
